**Quiz 5**

**(Sec B)**

1. Draw the transfer characteristic curve for an n-channel JFET using short hand method when Vp=-5 V and IDSS= 8 mA ( You may redraw the curve from Quiz 4), Find IDQ and VGSQ for a JFET self biased configuration circuit show below. Where RS=100 Ω.

